PAlib: PA9.h Source File

Main Page | Modules | File List | Globals | Search for

# PA9.h

Go to the documentation of this file.

    00001 #ifndef _PA_Main
    00002 #define _PA_Main
    00003
    00004 #ifdef __cplusplus
    00005 extern "C" {
    00006 #endif
    00007
    00008
    00009 #include "../../PA_Config.h"
    00010
    00011
    00012 #ifdef USE_8BITTEXT
    00013        #define TEXT_ALLSIZES
    00014 #endif
    00015
    00016
    00017 #include <nds.h>
    00018 #include <nds/memory.h>
    00019 #include <nds/bios.h>
    00020 #include <malloc.h>
    00021
    00022 extern bool PA_Screen;
    00023
    00024 typedef struct {
    00025    u8 NoIdea;
    00026    u8 Year;
    00027    u8 Month;
    00028    u8 Day;
    00029    u8 NoIdea2;
    00030    u8 Hour;
    00031    u8 Minutes;
    00032    u8 Seconds;
    00033 } RTC;
    00034 extern RTC PA_RTC;
    00035
    00036 extern inline void PA_WaitForVBL(void);
    00037
    00038 extern s16 PA_ScreenSpace; // Espace entre les 2 écrans...+192
    00039
    00040 #define BG_GFX1                    0x6000000
    00041 #define BG_GFX2                    0x6200000
    00042 #define SPRITE_GFX1         0x6400000
    00043 #define SPRITE_GFX2         0x6600000
    00044
    00045
    00046 //Pour le DMA Copy...
    00047 #define REG_DMA3SRC *(volatile u32*)0x040000D4
    00048 #define REG_DMA3DST *(volatile u32*)0x040000D8
    00049 #define REG_DMA3CNT *(volatile u32*)0x040000DC
    00050 #define DMA_ON 0x80000000
    00051 #define DMA_NOW 0x00000000
    00052 #define DMA_16 0x00000000
    00053 #define DMA_32 0x04000000
    00054 #define DMA_16NOW (DMA_ON | DMA_NOW | DMA_16)
    00055 #define DMA_32NOW (DMA_ON | DMA_NOW | DMA_32)
    00056 #define DMA_Copy(source, dest, count, mode) {REG_DMA3SRC = (u32)source; REG_DMA3DST = (u32)dest; REG_DMA3CNT = (count) | (mode);}
    00057
    00058 #define DMA_Clear(dest, count, mode) {REG_DMA3SRC = (u32)Blank; REG_DMA3DST = (u32)dest; REG_DMA3CNT = (count) | (mode);}
    00059
    00060 #define DMA_Force(ulVal,dest, count, mode) {REG_DMA3SRC=(u32)&ulVal; REG_DMA3DST = (u32)dest; REG_DMA3CNT = (count) |(mode) | DMA_SRC_FIX;}
    00061
    00062 // Commandes pour la lumière des écrans
    00063 #define BACKLIGHT(screen)   BIT(2+screen)
    00064
    00065
    00066
    00067
    00068
    00069
    00070
    00071 #include <stdarg.h> // Pour le système de text
    00072 #include <string.h>
    00073
    00074 #include "gbfs.h"
    00075 #include "gba-jpeg-decode.h"
    00076 #include "Sound9.h"
    00077
    00078
    00079 #define _REG8 *(volatile u16 *)
    00080 #define _REG16 *(volatile u16 *)
    00081 #define _REG32 *(volatile u32 *)
    00082
    00083 #include "arm9/vidfile.h"
    00084 #include "arm9/PA_Sprite.h"
    00085 #include "arm9/PA_SpriteDual.h"
    00086 #include "arm9/PA_Sound.h"
    00087 #include "arm9/PA_Micro.h"
    00088 #include "arm9/PA_Draw.h"
    00089 #include "arm9/PA_Interrupt.h"
    00090 #include "arm9/PA_Keys.h"
    00091
    00092 #include "arm9/PA_Timer.h"
    00093
    00094 #ifdef TEXT_ALLSIZES
    00095        #include "arm9/PA_API.h"  // API only if has text...
    00096 #endif
    00097
    00098 #include "arm9/PA_Math.h"
    00099 #include "arm9/PA_Palette.h"
    00100 #include "arm9/PA_PaletteDual.h"
    00101 #include "arm9/PA_Save.h"
    00102 #include "arm9/PA_FS.h"
    00103 #include "arm9/PA_GBFS.h"
    00104 #include "arm9/PA_SpecialFx.h"
    00105
    00106 #include "arm9/PA_Tile.h"
    00107 #include "arm9/PA_TileDual.h"
    00108
    00109 #include "arm9/PA_FAT.h"  // fat driver by chrishm
    00110
    00111 #ifdef USE_KEYBOARD
    00112        #include "arm9/PA_Keyboard.h"
    00113 #endif
    00114
    00115 #include "arm9/PA_Text.h"
    00116 #include "arm9/PA_Window.h"
    00117
    00118 #include "arm9/PA_Mode7.h"
    00119
    00120 #ifdef USE_3D
    00121        #include "arm9/PA_3D.h"
    00122 #endif
    00123
    00124
    00125 #include "arm9/PA_IA.h"
    00126 #include "arm9/PA_Reco.h"
    00127
    00128 #define SWITCH_SCREENS  (1<<15)
    00129
    00130
    00131
    00132 #define N_HBLS 263
    00133
    00134
    00135
    00144 //extern u32 *Blank;
    00145 extern u32 Blank[130000>>2];
    00146
    00147
    00148
    00149
    00150
    00151
    00153 // Général
    00155
    00156 #define SIZEOF_8BIT(x)          (sizeof(x))
    00157 #define SIZEOF_16BIT(x)         (sizeof(x)>>1)
    00158 #define SIZEOF_32BIT(x)         (sizeof(x)>>2)
    00159
    00160
    00161
    00162
    00163 #define CODE_IN_IWRAM __attribute__ ((section (".iwram"), long_call))
    00164 #define IN_IWRAM __attribute__ ((section (".iwram")))
    00165 #define CODE_IN_EWRAM __attribute__ ((section (".ewram"), long_call))
    00166 #define IN_EWRAM __attribute__ ((section (".ewram")))
    00167 #define PACKED __attribute__ ((packed))
    00168
    00169
    00170
    00171
    00172
    00173
    00174
    00175 // Jpeg functions :
    00176 void PA_jpeg_GetImageSize(char* name, int* width, int* height);
    00177 void PA_jpeg_BltImage(char* name, u16* vram, int output_width, int output_height);
    00178
    00179 extern const s16 PA_SIN[512];
    00180
    00181
    00182
    00183 typedef struct {
    00184    u8 Color;  // Favorite Color
    00185    u8 BdayMonth; // Mois d'anniversaire
    00186    u8 BdayDay;  // Jour de naissance
    00187    u8 AlarmHour;
    00188    u8 AlarmMinute;
    00189    u8 Name[21];
    00190    u8 NameLength;
    00191    u8 Message[53];
    00192    u8 MessageLength;
    00193    u8 Language; // Langue... 0 pour Jap, 1 pour anglais, 2 pour francais...
    00194 } infos;
    00195 extern infos PA_UserInfo;
    00196
    00197 #define INFO_COLOR *(u8*)0x027FFC82
    00198 #define INFO_BDAY_MONTH *(u8*)0x027FFC83
    00199 #define INFO_BDAY_DAY *(u8*)0x027FFC84
    00200 #define INFO_ALARM_HOUR *(u8*)0x027FFCD2
    00201 #define INFO_ALARM_MINUTE *(u8*)0x027FFCD3
    00202 #define INFO_NAME *(u8*)0x027FFC86
    00203 #define INFO_NAME_LENGTH *(u8*)0x027FFC9A
    00204 #define INFO_MESSAGE *(u8*)0x027FFC9C
    00205 #define INFO_MESSAGE_LENGTH *(u8*)0x027FFCD0
    00206 #define INFO_LANGUAGE  *(u8*)(0x027FFCE4)
    00207
    00208
    00220 void PA_Init(void);
    00221
    00222
    00223
    00235 extern inline void PA_SetVideoMode(bool screen, u8 mode) {
    00236        (*(vuint32*)(0x04000000 + (0x1000 * screen))) &= ~7;
    00237        (*(vuint32*)(0x04000000 + (0x1000 * screen))) |= mode;
    00238 }
    00239
    00240
    00241
    00247 void PA_UpdateUserInfo(void);
    00248
    00249
    00255 void PA_UpdateRTC(void);
    00256
    00257
    00265 void PA_LoadSplash(void);
    00266
    00267
    00273 void PA_NeoSplash(void);
    00274
    00275
    00276
    00282 extern inline void PA_WaitForVBL(void){
    00283 swiWaitForVBlank();
    00284 }
    00285
    00286
    00287
    00293 extern inline void PA_SwitchScreens(void) {
    00294 POWER_CR ^= SWITCH_SCREENS;
    00295 PA_Screen = !PA_Screen;
    00296 }
    00297
    00298
    00304 extern inline void PA_InitCPUMeter() {
    00305        PA_CPU = 0;
    00306        PA_MaxCPU = 0;
    00307        PA_lines = 0;
    00308        PA_VBLCount = 0;
    00309        PA_nVBLs = 0;
    00310 }
    00311
    00312
    00313
    00314
    00315
    00321 #define PA_LidClosed() (IPC->buttons>>7)
    00322
    00323
    00329 extern inline bool PA_CheckLid(void) {
    00330
    00331 if (!PA_LidClosed()) return 0;
    00332 else {
    00333        u16 power_cr = POWER_CR; // backup the power...
    00334        POWER_CR = 0; // Shutdown everything :p
    00335
    00336        // Wait for the lid to be opened again...
    00337        while(PA_LidClosed()) PA_WaitForVBL();
    00338
    00339        // Return the power !
    00340        POWER_CR = power_cr;
    00341        return 1;
    00342 }
    00343
    00344 }
    00345
    00346
    00347
    00348
    00349
    00377 void PA_Splash(void* tiles0, void* map0, void* tiles1, void* map1, s16 color0, s16 color1, s16 time);
    00378
    00379
    00391 extern inline void PA_SetScreenLight(bool screen, bool light){
    00392        IPC->aux &= ~(1<<(2+screen));
    00393        IPC->aux |= light<<(2+screen);
    00394 }
    00395
    00396
    00408 extern inline void PA_SetLedBlink(bool blink, bool speed){
    00409        IPC->aux &= ~(3<<4);
    00410        IPC->aux |= (blink + (speed<<1))<<4;
    00411 }
    00412
    00413
    00414
    00415  // end of General
    00417
    00418
    00419 void PA_Nothing(void);
    00420
    00421
    00422 #ifdef __cplusplus
    00423 }
    00424 #endif
    00425 #endif
    00426
    00427
    00428